VAS "Latvijas dzelzceļš" negotiation procedures with publication

"Delivery of spare parts for two-axle carriages of freight wagons for the needs of

SIA "LDZ rolling stock service"

**TECHNICAL SPECIFICATION**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Nr.** | **Spare parts** | **Technical characteristics of the product, drawings** | **Product's original manufacturing plants number** | **Product unit of measure** | **Total amount** | **The name of the product manufacturer and a reference to the manufacturer's document certifying compliance with the technical specification, indicating the exact page of the offer** |
|  |
| **Spare parts for 2-axle carts (type 2, GOST 9246) of freight wagons** |  |
| 1 | External spring | 100.30.018-0; 100.30.021-0; 7055.30.004-0; 9801.30.018; 1750.30.002; ЧЛЗ-100.50.002; 2128-07.50.00.002; 1272.304585.008  |  | pieces | 750 |   |  |
| 2 | Internal spring | 100.30.019-0; 100.30.022-0; 7055.30.005-0; 9801.30.019; 1750.30.004; ЧЛЗ-100.50.003; 2128-07.50.00.003; 1272.304585.007  |  | pieces | 750 |   |  |
| 3 | Gasket | M1698.01.005 |  | pieces | 300 |   |  |
| 4 | Sliding rim | M1698.01.100 СБ |  | pieces | 100 |   |  |
| 5 | Fixed friction plate (10mm) | M1698.02.001 |  | pieces | 800 |   |  |
| 6 | Movable friction plate (6 mm) | M1698.02.004 |  | pieces | 3 900 |   |  |
| 7 | Gasket | M1698.02.100СБ |  | pieces | 200 |   |  |
| 8 | Gasket | M1698.03.100СБ |  | pieces | 1 100 |   |  |
| 9 | Gear linkage roller 30x75 | 100.40.002-0  |  | pieces | 700 |   |  |
| 10 | brake linkage roller 90x30 | 100.40.003-0  |  | pieces | 300 |   |  |
| 11 | Gear linkage roller 40х75 | 100.40.004-0 |  | pieces | 1 500 |   |  |
| 12 | Suspension roller 30\*220 | 100.40.013-0 |  | pieces | 700 |   |  |
| 13 | Brake pad pin | 100.40.014-0  |  | pieces | 50 |   |  |
| 14 | rubber-metal element | 100.41.010-2СБ |  | pieces | 500 |   |  |
| 15 | Persistent rod | 100.41.020-1СБ |  | pieces | 50 |   |  |
| 16 | Polymer inserts Ø45 | 194.00.054-0  |  | pieces | 4 900 |   |  |
| 17 | Polymer inserts Ø46 | 194.00.054-0  |  | pieces | 400 |   |  |
| 18 | Composite brake pads | 25130-03-H; 2TP-11-01 |  | pieces | 8 400 |   |  |
| 19 | Safety brace | 4384.00.00  |  | pieces | 1 700 |   |  |

***With the offer, the applicant also submits:***

1. ***for each proposed negotiation procedure - item part/position, technical description of the product or quality certificate or passport issued by the manufacturer (drawing number, standard according to which the product is manufactured),*** *certifying the compliance of the product with the Technical Specification, together with information about the manufacturer's address, website address, e-mail address and contacts. If the offered product does not meet the specified standards, the applicant must submit the manufacturer's technical documentation and/or a certificate issued by a competent institution on the test results, which proves that the offered product is equivalent to that specified in the technical specification.*

*In the event that the product is available in the warehouse, the applicant indicates it in the technical offer, indicating the manufacturer of the relevant product (as well as attaching documents certifying the quality of the product);*

1. ***a copy of the certificate of conformity*** *for parts* ***1., 2. and 18. of the subject of the negotiation*** *procedure separately and a* ***copy of the declaration of conformity*** *for part* ***13.*** *of the subject of the negotiation procedure separately, which confirms the compliance of the goods with the Technical Specification.*

Conditions of other negotiation procedures and mandatory documents for participation in the procurement annex: “Kravas vagonu divasu ratiņu rezerves daļas piegāde SIA “LDZ ritošā sastāva serviss” vajadzībām”.